Spectrum TEZP-405-30 & TEZP-405-30-V1 2MP 40x Explosion Proof PTZ Network Camera

Certified (ATEX & IECEx Approved) for use in potentially combustible environments, this product is an explosion-proof PTZ camera delivering 60fps at 1080p resolution. It features a 40x optical zoom, 360° endless pan, and is enclosed in a 316L Stainless Steel housing. This model includes an integrated IR illuminator with a night distance of up to 200m.

• 1/2.8" Sony CMOS Sensor
• 40x Optical Zoom (4.25mm to 170.0mm)
• 32x Digital Zoom
• Digital Noise Reduction (DNR)
• Defog Function
• IR Night Distance up to 200m
• 255 Presets, 8 Tours, 4 Patterns
• 360° Endless Pan Rotation
• -90° to +90° Tilt
• 316L Stainless Steel Construction
• IP67
• H.265, H.264, MJPEG Triple Streams
• ONVIF Compatibility
• 5 Year Warranty

Model Power Variations
TEZP-405-30: 24VAC (Max 99W Camera, Max 50W IR)
TEZP-405-30-V1: 100-240VAC, Max 120W

Explosion-proof Certifications
ATEX & IECEx
Ex II 2 GD Ex db IIC T6 Gb
Ex tb IIIC T80°C Db
Ambient Temperature: Ta = -40°C to +60°C
IP Rating: IP67

Camera
Image Sensor: 1/2.8" Sony CMOS Sensor
Lens: 40x Day & Night Zoom Lens
Focal Length: F=4.25mm ~ 170.0mm
Aperture Ratio: F1.6 (Wide) ~ F4.95 (Tele)
Minimum illumination (Color): 0.01 lux / DSS 0.001 lux
Minimum illumination (B/W): 0.002 lux / DSS 0.0002 lux
Shutter speed: 1/30 (25) ~ 1/30,000 sec
WDR/BLC: Off / WDR / BLC / HLC / ACE
DNR (Digital Noise Reduction): Auto / Off / Low / Middle / High
Defog: On / Off

Pan/Tilt
Pan: 360° Continuous, 0.05° ~ 50°/Sec
Tilt: -90° ~ +90°, 0.1° ~ 50°/Sec
Preset: 255 Points

Video
Video Compression: H.265, H.264, M.JPEG
Resolution: 1920x1080, 1280x720, 1024x576, 640x360, D1, 4CIF, VGA, CIF, QVGA
Frame Rate (Max): Up to 60fps @ 1920x1080
Video Streaming: Supports up to Triple Streams

Network
Security: Multi-Level Security
Supported Protocols: HTTP, RTP/RTSP, TCP/IP (V4/V6), UDP, FTP, Telnet, HTTPS, SNMP, DHCP, NTP, SMTP, uPnP

General
Casing: Stainless Steel 316L
Weight: 79.4 lbs (36 kg)
Power Source (TEZP-405-30): 24VAC (Camera + IR)
Power Source (TEZP-405-30-V1): 100-240VAC, Max 120W
Operating Conditions: -40°C to 60°C (-40°F to 140°F), Humidity 0-95% RH
IP Rating: IP67
Warranty: 5-year warranty
Dimensions: 24.1(W) x 17.2(H) x 9.3(D) inches (611 x 438 x 235 mm)